**Rules Of the Road – For the Model “A” Ford**

1. **Following others** - NEVER follow too close. ALWAYS leave plenty of room to stop. Model “A” brakes leave a lot to be desired. Get them adjusted at least twice a year.
2. **Passing** – Only pass when you know you have **more room** **than you need. Speeding up and stopping in the “A” can be** difficult. Do not put yourself in an unsafe situation.
3. **Gas** - Always go out on tour with a FULL tank of gas.
4. **Turn outs** – Always use turn outs and get as far off the road as safely possible.
5. **Buddy System** – try to always travel with others – 2 or 3 cars
6. **Break Down** – if you or someone else breaks down get off the road. Have your buddy direct traffic if needed. Only have two cars stop…others go on to a safe stop. NEVER have too many cars pull off the road so you don’t create yet another hazard.
7. **Side Trips** – If you take a side trip or depart from the group notify others in the group.
8. **CB Radio** – if you have one we use channel 5.
9. **Departure Time** – we usually set a time to “gather” and a time to “depart”. Depart time is fixed and we go on time!
10. **Tour Leaders Cell phone** – ALWAYS get the leaders cell phone number.

**Things that are great to have with you as you tour:**

Coil Condenser Set of Points

Fan Belt Amp Meter Cut out for Generator

Jack Hand Crank Water Pump

Distributor Carburetor Front Outer Wheel Bearing

Socket Set Screwdriver Plyers

Quart of Oil Feeler Gauge Crescent Wrench

Grease gun End Wrenches Fire Extinguisher!

Repair Manual Gallon of Water Money for a Hotel Room! ☺

Revised: 12/12/12